**Setting Up The NanoPi 2 From Start to Finish**

April 25, 2017

Index:

1. Node
2. Serial Port
3. Git
4. Kweb (Minimal Kiosk Browser)
5. **Install Node**

Reference: <https://github.com/nodesource/distributions>

Enter these commands:

curl -sL <https://deb.nodesource.com/setup_7.x> | sudo -E bash -

sudo apt-get install -y nodejs

To check installation: node -v

1. **Install Serial port (from npm.js)**

sudo apt-get update

sudo apt-get install build-essential

npm install serialport

There could be some error messages – this seems to be OK

1. **Install GIT**

sudo apt-get install git

1. **Install KWEB**

Reference: <https://www.raspberrypi.org/forums/viewtopic.php?t=40860>

wget <http://steinerdatenbank.de/software/kweb-1.7.8.tar.gz>

tar -xzf kweb-1.7.8.tar.gz

cd kweb-1.7.8

./debinstall **Setting Up The NanoPi 2 From Start to Finish**

April 25, 2017

**Index:**

0.    Install operating system

1.      Node

2.      Serial Port

3.      Git

4.      Kweb (Minimal Kiosk Browser)

5.    Samba

6.    Audio

7.    Screen

8.    Autorun program

**0. Install operating system**

Download: 5p4418-eflasher-sd8g-xxx-full.img.7z  from this website: <https://www.mediafire.com/folder/ilkcy37otd7il/S5P4418>

Unzip and then usw win32DiskImager to write to micrdSD card

Instal sdl in NanoPi S2, hold the boot button and then power on.

Select operating system and wait.

**1.** **Install Node**

Reference:  <https://github.com/nodesource/distributions>

Enter these commands:

curl -sL<https://deb.nodesource.com/setup_7.x> | sudo -E bash -

sudo apt-get install -y nodejs

To check installation: node -v

**2.** **Install Serial port (from npm.js)**

sudo apt-get update

sudo apt-get install build-essential

npm install serialport

           There could be some error messages – this seems to be OK

**3.** **Install GIT - and project**

sudo apt-get install git

git clone <https://github.com/level451/r5.git>

cd r5

npm update

**4.** **Install Chromium**

sudo apt-get update

wget -qO - http://bintray.com/user/downloadSubjectPublicKey?username=bintray | sudo apt-key add -

echo "deb http://dl.bintray.com/kusti8/chromium-rpi jessie main" | sudo tee -a /etc/apt/sources.list

sudo apt-get update

sudo apt-get install chromium-browser

**5. Install SMB – using Samba**

sudo apt-get update

           sudo apt-get install samba  (accept prompt)

sudo apt-get install samba-common-bin

sudo nano /etc/samba/smb.conf

                then:

**Add to bottom of file::**

[nanohome]

path=/home/fa

read only = no

writable = yes

browseable = yes

guest ok = yes

create mask = 0755

directory mask = 0755

public = yes

[nanoroot]

comment = Nano root

path=/

Writeable = Yes

browseable=Yes

only guest=no

create mask=0777

directory mask=0777

public=yes

then save

set up password:  sudo smbpasswd -a root

Do a restart just to make sure:  sudo /etc/init.d/samba restart

TO REMOVE SAMBA: sudo apt-get purge samba

**6. Install Audio**

**apt-get update**  
 **apt-get install** libasound2  
 **apt-get install** alsa-base  
 **apt-get install** alsa-utils

**7. Install Screen**

sudo apt-get install screen

These are the commands to use screen:

screen –ls to see all running screens

screen –r (name) to go to a screen

screen exit to exit and kill processes running on that screen

**8. Autorun program**

**Do Parts 1 and 2!**

**Part 1:**

Auto run on boot script file:

create file:   sudo nano /etc/init.d/autorun.sh

copy contents between the dashed lines and save it

Then:    cd /etc/init.d

           sudo chmod 755 autorun.sh

To make auto start:  sudo update-rc.d autorun.sh defaults

----------------------------------------------

### BEGIN INIT INFO

# Provides:          autorun.sh

# Required-Start:    $all

# Required-Stop:     $all

# Default-Start:     2 3 4 5

# Default-Stop:      0 1 6

# Short-Description: Short script description

# Description:       Longer script description.

### END INIT INFO

cd /root/r5

screen  -d -m -S r6 bash -c "sudo /usr/bin/node /home/fa/r5/app.js; exec bash"

echo  "Started R6"

------------------------------------------------------------

**Part 2**:

sudo nano /etc/xdg/lxsession/LXDE/autostart

Insert: @/etc/init.d/autorun.sh , before the screensaver line:

**HELPFUL HINTS:**

**To Stop node program: killall node**

**To close chromium-browser in kiosk mode: ALT-F4**